**M3901 SP\_Flash\_Tool USB Upgrade Instructions**

Please make sure to install the USB driver before upgrading. If it is not installed, install the SP\_Drivers driver according to the 3901 item USB driver manual in \Upgrade\DriverInstall.exe.


**Upgrade method**

upgrade tools：SP\_Flash\_Tool\_exe\_Windows\_v5.1748.00.000\flash\_tool.exe


**Upgrade scenario**

1. In the USB upgrade package Download\_Tool file, double-click to open the Flash tool tool.


Download-Agent selects "MTK\_AllInOne\_DA.bin" by default, as shown in the figure.。




1. Scatter-loading File selects "MT6739\_Android\_scatter.txt" , as shown in the figure.



1. The upgrade method selects the third item of the pull-down menu, which is "Firmware Upgrade", as shown in the figure.



1. Click Download。



4. After the phone is turned off, connect the USB cable to upgrade. The upgrade is successful.

